Version: 2

Offset: 240
Pin: pwrup_rst_n W MET4

Spacing: 120
Pin: rst_n W MET4
Pin: cpu_rst_n W MET4
Pin: test_mode W MET4
Pin: test_rst_n W MET4
Pin: clk W MET4
Pin: rtc_clk W MET4
Pin: sys_rst_n_o W MET4
Pin: sys_rdc_qlfy_o W MET4
Pin: fuse_mhartid[31] W MET4
Pin: fuse_mhartid[30] W MET4
Pin: fuse_mhartid[29] W MET4
Pin: fuse_mhartid[28] W MET4
Pin: fuse_mhartid[27] W MET4
Pin: fuse_mhartid[26] W MET4
Pin: fuse_mhartid[25] W MET4
Pin: fuse_mhartid[24] W MET4
Pin: fuse_mhartid[23] W MET4
Pin: fuse_mhartid[22] W MET4
Pin: fuse_mhartid[21] W MET4
Pin: fuse_mhartid[20] W MET4
Pin: fuse_mhartid[19] W MET4
Pin: fuse_mhartid[18] W MET4
Pin: fuse_mhartid[17] W MET4
Pin: fuse_mhartid[16] W MET4
Pin: fuse_mhartid[15] W MET4
Pin: fuse_mhartid[14] W MET4
Pin: fuse_mhartid[13] W MET4
Pin: fuse_mhartid[12] W MET4
Pin: fuse_mhartid[11] W MET4
Pin: fuse_mhartid[10] W MET4
Pin: fuse_mhartid[9] W MET4
Pin: fuse_mhartid[8] W MET4
Pin: fuse_mhartid[7] W MET4
Pin: fuse_mhartid[6] W MET4
Pin: fuse_mhartid[5] W MET4
Pin: fuse_mhartid[4] W MET4
Pin: fuse_mhartid[3] W MET4
Pin: fuse_mhartid[2] W MET4
Pin: fuse_mhartid[1] W MET4
Pin: fuse_mhartid[0] W MET4
Pin: fuse_idcode[31] W MET4
Pin: fuse_idcode[30] W MET4
Pin: fuse_idcode[29] W MET4
Pin: fuse_idcode[28] W MET4
Pin: fuse_idcode[27] W MET4
Pin: fuse_idcode[26] W MET4
Pin: fuse_idcode[25] W MET4
Pin: fuse_idcode[24] W MET4
Pin: fuse_idcode[23] W MET4
Pin: fuse_idcode[22] W MET4
Pin: fuse_idcode[21] W MET4
Pin: fuse_idcode[20] W MET4
Pin: fuse_idcode[19] W MET4
Pin: fuse_idcode[18] W MET4
Pin: fuse_idcode[17] W MET4
Pin: fuse_idcode[16] W MET4
Pin: fuse_idcode[15] W MET4
Pin: fuse_idcode[14] W MET4
Pin: fuse_idcode[13] W MET4
Pin: fuse_idcode[12] W MET4
Pin: fuse_idcode[11] W MET4
Pin: fuse_idcode[10] W MET4
Pin: fuse_idcode[9] W MET4
Pin: fuse_idcode[8] W MET4
Pin: fuse_idcode[7] W MET4
Pin: fuse_idcode[6] W MET4
Pin: fuse_idcode[5] W MET4
Pin: fuse_idcode[4] W MET4
Pin: fuse_idcode[3] W MET4
Pin: fuse_idcode[2] W MET4
Pin: fuse_idcode[1] W MET4

Offset: 240
Pin: fuse_idcode[0] S MET4

Spacing: 120
Pin: irq_lines[15] S MET4
Pin: irq_lines[14] S MET4
Pin: irq_lines[13] S MET4
Pin: irq_lines[12] S MET4
Pin: irq_lines[11] S MET4
Pin: irq_lines[10] S MET4
Pin: irq_lines[9] S MET4
Pin: irq_lines[8] S MET4
Pin: irq_lines[7] S MET4
Pin: irq_lines[6] S MET4
Pin: irq_lines[5] S MET4
Pin: irq_lines[4] S MET4
Pin: irq_lines[3] S MET4
Pin: irq_lines[2] S MET4
Pin: irq_lines[1] S MET4
Pin: irq_lines[0] S MET4
Pin: ext_irq S MET4
Pin: soft_irq S MET4
Pin: trst_n S MET4
Pin: tck S MET4
Pin: tms S MET4
Pin: tdi S MET4
Pin: tdo S MET4
Pin: tdo_en S MET4
Pin: imem_hprot[3] S MET4
Pin: imem_hprot[2] S MET4
Pin: imem_hprot[1] S MET4
Pin: imem_hprot[0] S MET4
Pin: imem_hburst[2] S MET4
Pin: imem_hburst[1] S MET4
Pin: imem_hburst[0] S MET4
Pin: imem_hsize[2] S MET4
Pin: imem_hsize[1] S MET4
Pin: imem_hsize[0] S MET4
Pin: imem_htrans[1] S MET4
Pin: imem_htrans[0] S MET4
Pin: imem_hmastlock S MET4
Pin: imem_haddr[31] S MET4
Pin: imem_haddr[30] S MET4
Pin: imem_haddr[29] S MET4
Pin: imem_haddr[28] S MET4
Pin: imem_haddr[27] S MET4
Pin: imem_haddr[26] S MET4
Pin: imem_haddr[25] S MET4
Pin: imem_haddr[24] S MET4
Pin: imem_haddr[23] S MET4
Pin: imem_haddr[22] S MET4
Pin: imem_haddr[21] S MET4
Pin: imem_haddr[20] S MET4
Pin: imem_haddr[19] S MET4
Pin: imem_haddr[18] S MET4
Pin: imem_haddr[17] S MET4
Pin: imem_haddr[16] S MET4
Pin: imem_haddr[15] S MET4
Pin: imem_haddr[14] S MET4
Pin: imem_haddr[13] S MET4
Pin: imem_haddr[12] S MET4
Pin: imem_haddr[11] S MET4
Pin: imem_haddr[10] S MET4
Pin: imem_haddr[9] S MET4
Pin: imem_haddr[8] S MET4
Pin: imem_haddr[7] S MET4
Pin: imem_haddr[6] S MET4
Pin: imem_haddr[5] S MET4
Pin: imem_haddr[4] S MET4
Pin: imem_haddr[3] S MET4
Pin: imem_haddr[2] S MET4
Pin: imem_haddr[1] S MET4
Pin: imem_haddr[0] S MET4
Pin: imem_hready S MET4
Pin: imem_hrdata[31] S MET4

Offset: 240
Pin: imem_hrdata[30] E MET4

Spacing: 120
Pin: imem_hrdata[29] E MET4
Pin: imem_hrdata[28] E MET4
Pin: imem_hrdata[27] E MET4
Pin: imem_hrdata[26] E MET4
Pin: imem_hrdata[25] E MET4
Pin: imem_hrdata[24] E MET4
Pin: imem_hrdata[23] E MET4
Pin: imem_hrdata[22] E MET4
Pin: imem_hrdata[21] E MET4
Pin: imem_hrdata[20] E MET4
Pin: imem_hrdata[19] E MET4
Pin: imem_hrdata[18] E MET4
Pin: imem_hrdata[17] E MET4
Pin: imem_hrdata[16] E MET4
Pin: imem_hrdata[15] E MET4
Pin: imem_hrdata[14] E MET4
Pin: imem_hrdata[13] E MET4
Pin: imem_hrdata[12] E MET4
Pin: imem_hrdata[11] E MET4
Pin: imem_hrdata[10] E MET4
Pin: imem_hrdata[9] E MET4
Pin: imem_hrdata[8] E MET4
Pin: imem_hrdata[7] E MET4
Pin: imem_hrdata[6] E MET4
Pin: imem_hrdata[5] E MET4
Pin: imem_hrdata[4] E MET4
Pin: imem_hrdata[3] E MET4
Pin: imem_hrdata[2] E MET4
Pin: imem_hrdata[1] E MET4
Pin: imem_hrdata[0] E MET4
Pin: imem_hresp E MET4
Pin: dmem_hprot[3] E MET4
Pin: dmem_hprot[2] E MET4
Pin: dmem_hprot[1] E MET4
Pin: dmem_hprot[0] E MET4
Pin: dmem_hburst[2] E MET4
Pin: dmem_hburst[1] E MET4
Pin: dmem_hburst[0] E MET4
Pin: dmem_hsize[2] E MET4
Pin: dmem_hsize[1] E MET4
Pin: dmem_hsize[0] E MET4
Pin: dmem_htrans[1] E MET4
Pin: dmem_htrans[0] E MET4
Pin: dmem_hmastlock E MET4
Pin: dmem_haddr[31] E MET4
Pin: dmem_haddr[30] E MET4
Pin: dmem_haddr[29] E MET4
Pin: dmem_haddr[28] E MET4
Pin: dmem_haddr[27] E MET4
Pin: dmem_haddr[26] E MET4
Pin: dmem_haddr[25] E MET4
Pin: dmem_haddr[24] E MET4
Pin: dmem_haddr[23] E MET4
Pin: dmem_haddr[22] E MET4
Pin: dmem_haddr[21] E MET4
Pin: dmem_haddr[20] E MET4
Pin: dmem_haddr[19] E MET4
Pin: dmem_haddr[18] E MET4
Pin: dmem_haddr[17] E MET4
Pin: dmem_haddr[16] E MET4
Pin: dmem_haddr[15] E MET4
Pin: dmem_haddr[14] E MET4
Pin: dmem_haddr[13] E MET4
Pin: dmem_haddr[12] E MET4
Pin: dmem_haddr[11] E MET4
Pin: dmem_haddr[10] E MET4
Pin: dmem_haddr[9] E MET4
Pin: dmem_haddr[8] E MET4
Pin: dmem_haddr[7] E MET4
Pin: dmem_haddr[6] E MET4
Pin: dmem_haddr[5] E MET4

Offset: 240
Pin: dmem_haddr[4] N MET4

Spacing: 120
Pin: dmem_haddr[3] N MET4
Pin: dmem_haddr[2] N MET4
Pin: dmem_haddr[1] N MET4
Pin: dmem_haddr[0] N MET4
Pin: dmem_hwrite N MET4
Pin: dmem_hwdata[31] N MET4
Pin: dmem_hwdata[30] N MET4
Pin: dmem_hwdata[29] N MET4
Pin: dmem_hwdata[28] N MET4
Pin: dmem_hwdata[27] N MET4
Pin: dmem_hwdata[26] N MET4
Pin: dmem_hwdata[25] N MET4
Pin: dmem_hwdata[24] N MET4
Pin: dmem_hwdata[23] N MET4
Pin: dmem_hwdata[22] N MET4
Pin: dmem_hwdata[21] N MET4
Pin: dmem_hwdata[20] N MET4
Pin: dmem_hwdata[19] N MET4
Pin: dmem_hwdata[18] N MET4
Pin: dmem_hwdata[17] N MET4
Pin: dmem_hwdata[16] N MET4
Pin: dmem_hwdata[15] N MET4
Pin: dmem_hwdata[14] N MET4
Pin: dmem_hwdata[13] N MET4
Pin: dmem_hwdata[12] N MET4
Pin: dmem_hwdata[11] N MET4
Pin: dmem_hwdata[10] N MET4
Pin: dmem_hwdata[9] N MET4
Pin: dmem_hwdata[8] N MET4
Pin: dmem_hwdata[7] N MET4
Pin: dmem_hwdata[6] N MET4
Pin: dmem_hwdata[5] N MET4
Pin: dmem_hwdata[4] N MET4
Pin: dmem_hwdata[3] N MET4
Pin: dmem_hwdata[2] N MET4
Pin: dmem_hwdata[1] N MET4
Pin: dmem_hwdata[0] N MET4
Pin: dmem_hready N MET4
Pin: dmem_hrdata[31] N MET4
Pin: dmem_hrdata[30] N MET4
Pin: dmem_hrdata[29] N MET4
Pin: dmem_hrdata[28] N MET4
Pin: dmem_hrdata[27] N MET4
Pin: dmem_hrdata[26] N MET4
Pin: dmem_hrdata[25] N MET4
Pin: dmem_hrdata[24] N MET4
Pin: dmem_hrdata[23] N MET4
Pin: dmem_hrdata[22] N MET4
Pin: dmem_hrdata[21] N MET4
Pin: dmem_hrdata[20] N MET4
Pin: dmem_hrdata[19] N MET4
Pin: dmem_hrdata[18] N MET4
Pin: dmem_hrdata[17] N MET4
Pin: dmem_hrdata[16] N MET4
Pin: dmem_hrdata[15] N MET4
Pin: dmem_hrdata[14] N MET4
Pin: dmem_hrdata[13] N MET4
Pin: dmem_hrdata[12] N MET4
Pin: dmem_hrdata[11] N MET4
Pin: dmem_hrdata[10] N MET4
Pin: dmem_hrdata[9] N MET4
Pin: dmem_hrdata[8] N MET4
Pin: dmem_hrdata[7] N MET4
Pin: dmem_hrdata[6] N MET4
Pin: dmem_hrdata[5] N MET4
Pin: dmem_hrdata[4] N MET4
Pin: dmem_hrdata[3] N MET4
Pin: dmem_hrdata[2] N MET4
Pin: dmem_hrdata[1] N MET4
Pin: dmem_hrdata[0] N MET4
Pin: dmem_hresp N MET4



#                                    clk    rtc_clk    fuse_mhartid[31:0]    fuse_idcode[31:0]    
#                      -----------------------------------------------------------------------------------------
#trst_n                |                                                                                       |    sys_rst_n_o
#tck                   |                                                                                       |    sys_rdc_qlfy_o
#tms                   |                                                                                       |
#tdi                   |                                                                                       |
#                      |                                                                                       |
#tdo                   |                                                                                       |
#tdo_en                |                                                                                       |    dmem_hready
#                      |                                                                                       |    dmem_hrdata[31:0]
#imem_hready           |                                                                                       |    dmem_hresp
#imem_hrdata[31:0]     |                                                                                       |
#imem_hresp            |                                                                                       |    dmem_hprot[3:0]
#                      |                                                                                       |    dmem_hburst[2:0]
#imem_hprot[3:0]       |                                                                                       |    dmem_hsize[2:0]
#imem_hburst[2:0]      |                                                                                       |    dmem_htrans[1:0]
#imem_hsize[2:0]       |                                                                                       |    dmem_hmastlock
#imem_htrans[1:0]      |                                                                                       |    dmem_haddr[31:0]
#imem_hmastlock        |                                                                                       |    dmem_hwrite
#imem_haddr[31:0]      |                                                                                       |    dmem_hwdata[31:0]
#                      -----------------------------------------------------------------------------------------
#                                              irq_lines[15:0]    ext_irq    soft_irq                             



# pwrup_rst_n
# rst_n
# cpu_rst_n
# test_mode
# test_rst_n
# clk
# rtc_clk
# sys_rst_n_o
# sys_rdc_qlfy_o
# fuse_mhartid[31:0]
# fuse_idcode[31:0]
# irq_lines[15:0]
# ext_irq
# soft_irq
# trst_n
# tck
# tms
# tdi
# tdo
# tdo_en
# imem_hprot[3:0]
# imem_hburst[2:0]
# imem_hsize[2:0]
# imem_htrans[1:0]
# imem_hmastlock
# imem_haddr[31:0]
# imem_hready
# imem_hrdata[31:0]
# imem_hresp
# dmem_hprot[3:0]
# dmem_hburst[2:0]
# dmem_hsize[2:0]
# dmem_htrans[1:0]
# dmem_hmastlock
# dmem_haddr[31:0]
# dmem_hwrite
# dmem_hwdata[31:0]
# dmem_hready
# dmem_hrdata[31:0]
# dmem_hresp


















